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SECTION 1. GENERAL INFORMATION
	Subsection 1.1. Procurement item

	The delivery of additional personal protection equipment (PPE) (hereinafter the Goods) and requirements for them are given in Annex No. 1 to the Technical Assignment viz. "Specification of the goods" (hereinafter the Specification).

	Subsection 1.2. Novelty information

	The delivered goods must be new, manufactured not earlier than 2025, not used, not restored, not be exhibition samples, free from the rights of any third parties, if not specified otherwise in the Specification.

	Subsection 1.3. OKPD-2

	The OKPD-2 codes are specified in the Specification.


SECTION 2. SCOPE OF APPLICATION
	Providing AKKUYU NÜKLEER ANONİM ŞİRKETİ employees with personal protection equipment (PPE). The goods are designed for daily use (application) at the production areas and territories where there are general purpose industrial grade impurities, risks of mechanical action, as well as for operation in the areas requiring the use of additional PPE against the risks of fall from height


SECTION 3. OPERATING CONDITIONS
	Heated and unheated rooms, as well as outdoors.


SECTION 4. TECHNICAL REQUIREMENTS
	Subsection 4.1. Main parameters and dimensions

	The Goods to be supplied shall comply with all requirements indicated in the Specification.
The brand logos placed on the ready-made goods from the sub-item 1,2, 3 of the Specification are given in Appendix No. 2 to this TA.

	Subsection 4.2. Reliability requirements

	The design, manufacturing quality of the Goods and used materials shall ensure reliable operation during the entire operating period.

	Subsection 4.3. Requirements for materials and components

	Requirements for materials and components of the purchased items are stated in the Specification.

	Subsection 4.4. Power requirements

	Not required 

	Subsection 4.5. Requirements for power consumption, power saving and energy efficiency

	Not required 

	Subsection 4.6. Requirements for completeness

	The completeness requirements have been specified in the Specification.

	Subsection 4.7. Marking requirements

	4.7.1 The PPE marking shall be applied directly to the PPE or on a difficult-to-remove label attached to the product. The information on the PPE label must be exhaustive, accurate, easy to read, clearly printed with indelible paint, and durable throughout the life of the product during storage and operation. The PPE label shall bear the European Quality Certificate - CE for EU countries and contain information about:
1)	the manufacturer;
2)	the product name;
3)	the protective properties (with indication of maximum values);
4)	the size;
5)	the manufacturing date.
6) 	 All products must comply with current European or Turkish standards (EN, ISO, TSE).


	Subsection 4.8. Packing requirements 

	The Goods shall be supplied in company packing (considering the required markings), the packing should provide the quality and safety of the goods during transportation up to the destination point considering the overloads, and during subsequent storage.
The packing shall clearly indicate: the manufacturing date, shelf life, batch number (serial number) in accordance with the requirements of the Specification, and manufacturer’s data.
The packing of the delivered Product shall not have any external defects and traces of opening, must comply with the requirements of life safety, health and environmental protection, have the necessary markings, labels, seals, and also provide the possibility to determine the quantity of the items contained in it (description, packaging labels or sheets).


SECTION 5. ACCEPTANCE REQUIREMENTS
	Subsection 5.1. Acceptance procedure

	5.1.1. The Goods shall be accepted at the Buyer's premises at the following address: Republic of Türkiye, Akkuyu NPP construction site, Büyükeceli quarter, Akkuyu street, No. 3 A, Gülnar/Mersin (Akkuyu NPP construction industrial site, warehouse specified by the Buyer).
5.1.2 Acceptance of the Goods by quantity, completeness and quality shall be made within 10 (ten) business days from the date of actual delivery of the Goods to the Buyer, except in cases where additional tests of PPE are carried out at the TF (TL) under incoming inspection. In such cases, the PPE incoming inspection time shall be extended for the test duration of the PPE at the TF (TL). No additional tests are carried out for PPE RS that have passed the incoming inspection at the procurement stage. 
5.1.3 Based on the results of acceptance by quantity, completeness and quality of the Goods, the Buyer shall sign the Incoming Inspection Certificate of the PPE batch delivered, after which the Buyer shall notify the Supplier about the results of the incoming inspection of PPE carried out.
5.1.4 In the event that the Goods correspond to quantity, completeness and quality, the Supplier shall send  to the Buyer the Delivery and Acceptance Certificate for the delivered PPE, the Goods which have been delivered in terms of quantity, completeness and quality.
5.1.5 In the event that the Goods do not correspond to the quantity, completeness and quality, the Buyer shall issue the corresponding Fault Detection Report, the order is determined by the clause 6.20 of the Contract.
5.1.6 The Goods shall not be accepted in case of inconsistency of the invoice and list of the delivered Goods, if they shall be counterfeit, adulterated Goods and Goods of dubious origin.
5.1.7 If any discrepancy is detected in the quantity, completeness and quality of the Goods, the Supplier shall be obliged at its own expense and risk to additionally deliver the Goods, complete the incomplete Goods or replace them, without prejudice to the rights of the Buyer. The Buyer shall have the sole right to choose the method of reconciling with the discrepancy.

	Subsection 5.2. Requirements for transfer of the technical and other documents to the Customer during delivery of the goods

	5.2.1 The Supplier shall provide the following supporting and operating documentation together with the Goods for each consignment separately:
a. Goods Delivery and Acceptance Certificate in 2 (two) original copies in the Turkish language along with the translation into Russian (one copy for the Buyer and one copy for the Supplier).
b. Consignment notes in 2 original copies in Turkish along with Russian translation (one copy for the Buyer and one copy for the Supplier).
c. Commercial invoice (if any).
d. Technical Data Sheet for the Goods or any other document containing all essential technical  characteristics of the Goods in Russian, English and/or in Turkish;
e. User manual or operation manual (if any) in Russian, English and/or Turkish.
f. Manufacturer's Warranty (warranty certificate or warranty booklet) issued in accordance with the procedure established by the manufacturer.
g. certification documents of the Goods (safety certificates, fire safety certificates, certificates of conformity or declaration of conformity, sanitary and hygiene certificates, environmental certificates), if the Goods are subject to certification in accordance with the law of the Republic of Türkiye.
5.2.2 The delivery of the Goods may include other mandatory, manufacturer-specific documentation required during operation.
5.2.3 The Supplier shall be liable for defects of the Goods unless it proves that these defects occurred after the delivery of the Goods to the Buyer due to the Buyer's violation of the conditions for storage of the Goods or actions of the third parties. Acceptance of the delivered Goods in terms of quantity and assortment shall be carried out by the Buyer at the time of delivery and acceptance of the Goods at the address specified in the Technical Assignment in accordance with terms and conditions hereof. 



SECTION 6. TRANSPORTATION REQUIREMENTS 
	The Supplier shall deliver the Goods to the Buyer by using its own vehicles or engaging third-party vehicles at the Supplier's expense, using the enclosed vehicles that preclude the possibility of external factors affecting the Goods. In case of delivery of the Goods from abroad, the Supplier shall provide customs clearance of the export of the Goods in the country of dispatch, transit, and clearance of the Goods under the customs procedure for release for domestic consumption in the Republic of Türkiye at its own expense.  All types of loading-and-unloading operations required for delivery of the Goods to the Place of delivery of the Goods (in accordance with clause 5.1 of this Technical Assignment), including operations to unload the Goods at the Place of Delivery, are performed by the Supplier using its own equipment and at its own expense. 
Packing, procedures for handling and transportation shall exclude the possibility of damage to the delivered Goods.
The transportation of Goods shall be allowed by railway and/or motor and/or air and/or sea transport to any distances.
The conditions of transport in terms of the exclusion of the influence of mechanical factors on the Goods should correspond to rail, air, road and sea transport respectively.
The Supplier shall be held liable for the sufficiency and reliability of the Goods packing during transportation.


SECTION 7. STORAGE REQUIREMENTS
	The Goods shall be stored in accordance with the manufacturer's recommendations specified in the data sheet (or other manufacturer's document).
If there are no storage requirements in the Specification, the storage conditions of the Goods shall be suitable for a tropical climate.


SECTION 8. REQUIREMENTS FOR THE SCOPE AND/OR PERIOD OF WARRANTY
	The warranty period for the delivered Goods must correspond to the period set by the manufacturer, but not less than 12 (twelve) months from the date of transfer of the Goods according to the Certificate or the Consignment Note.
The Supplier shall provide a guarantee of proper quality for the Goods for a period within the warranty period established by the manufacturer (in the documents for the goods providing for the warranty period) but not less than 12 (twelve) months from the date of transfer of the goods according to the Certificate or the Consignment Note.
The Supplier is obliged, during the warranty period, to replace the defective Goods with a new similar product of proper quality or a new product with the best technical and/or operational characteristics within the deadline agreed with the Buyer, if warranty repairs are impossible or troubleshooting (defect) will require significant time, as well as in the case of a malfunction occurs three or more times.


SECTION 9. SAFETY REQUIREMENTS
	Not required 


SECTION 10. MAINTENANCE REQUIREMENTS
	Not required


SECTION 11. ENVIRONMENTAL REQUIREMENTS
	Impact of this group of goods on the environment shall not exceed the values established by the current regulatory documents of the Republic of Türkiye. 


SECTION 12. SAFETY REQUIREMENTS
	•	All the delivered personal protection equipment (PPE) must comply with the requirements of Law No. 6331 "On occupational safety and health" and current regulatory acts of the Republic of Türkiye.
•	Products must provide adequate protection for employees against mechanical, chemical, thermal, electrical, biological and physical risks in accordance with the operating conditions.
•	For each type of PPE, a protection level or class that corresponds to the nature of the work to be performed and the degree of risk must be defined and indicated.
•	Design and materials of PPE must be ergonomic, not cause discomfort during prolonged wear, and not create additional health risks.
•	Protective equipment must be compatible when used simultaneously (e.g. helmet, goggles, respirator, headphones, etc.).
•	The Supplier is obliged to provide instructions for the operation, maintenance, cleaning, storage and periodic inspection of the products.
•	All products must be capable of safe replacement in the event of damage.
     •	The Goods shall not constitute a source of hazardous or harmful production factors or cause of accidents during operation.
All polymer materials used for personal protection equipment (PPE) shall be registered with the European Chemicals Agency (ECHA) under the REACH program (Registration, Evaluation, Authorization and Restriction of Chemicals). The certificates for the product should include information on registration of materials at ECHA in accordance with the "Rules for using personal protection equipment at workplaces" No. 28695 dated 02.07.2013.


SECTION 13. QUALITY REQUIREMENTS 
	The Goods must have CE quality assurance. The delivered Goods shall comply with the requirements specified in this Technical Assignment. 
The Goods shall be delivered in serviceable condition and in full compliance with the technical characteristics of the manufacturer.
The Supplier shall be fully responsible for quality of the delivered Goods.


SECTION 14. TECHNICAL SUPPORT OF GOODS
	Not required 


SECTION 15. ADDITIONAL (OTHER) REQUIREMENTS
	15.1 In order to assess the Participant’s ability to manufacture/deliver the Goods specified in Appendix 1 of the Technical Assignment to this TA, as well as its ability to supply all the necessary nomenclature and evaluate the quality of the specified samples, the Participant shall be obliged to submit samples for PPE (1 (one) unit each for the position 1 to 9 in accordance with Appendix 1 of the Technical Assignment "Specification"), as well as supporting and operating documentation (certificates of conformity, test reports, technical specifications, catalog of goods offered for delivery and photographs of samples provided). 
PPE RS provision procedure:
Deadline for the provision of reference samples to the bidders - no more than 10 calendar days from the end of the deadline for submission of bids by the bidders at the following address: Republic of Türkiye, Akkuyu NPP construction site, Büyükeceli quarter, Akkuyu street, 3 A, Gülnar/Mersin (NPP construction industrial site.
In order to arrange for the transfer of the PPE RS to the Procurement Participant, no later than 5 (five) business days prior to the expected date of transfer of the PPE Reference Samples (RS), send a request for provision of PPE RS by sending an e-mail letter according to the form in accordance with Annex No. 4 to this Technical Assignment to Tamara Yilmaz, Procurement Procedure Supervisor T.Yilmaz@akkuyu.com and to the official e-mail address of Buyer office@akkuyu.com.
In order to issue the Material Pass for the Reference Samples, the Bidder must provide the following information in a written notification (Annex No. 4 to this Technical Assignment):
1.	Goods Description;
2.	Number of reference samples for each position;
3.	Exact submission period of the reference samples (date, time);
4.	Purpose of reference samples (tests, conformity check, approval).
Upon receipt of confirmation of the readiness of material pass by the designated person, a notification is sent to the bidders by e-mail on the need to provide samples at the entry control point of the Akkuyu NPP construction site no later than 3 (three) business days after the receipt of the notification. 

The reference samples shall be provided in the quantity and within the time limits specified in the notification.
Each reference sample shall be accompanied by:
•	valid certificates of conformity and/or declaration of conformity;
•	quality data sheet / technical data sheet;
•	test records (if any);
An itemized inventory of the samples provided on the Bidder's letterhead shall be handed over with the samples. 
Copies of certificates of conformity for the PPE provided shall be submitted together with the PPE samples, certified by the procurement bidder.
The reference samples provided without written notice, with failure to meet the time limits, incomplete or without supporting documentation are not considered and may be the grounds for rejection of the Participant's offer.
PPE RS verification procedure: 
The samples shall be subject to expert review, for which reason their integrity may be violated. Submitted samples will be evaluated for compliance with the requirements of this Technical Assignment.
Expert assessment of the PPE samples shall be carried out by a committee with mandatory participation of occupational health specialists within 10 (ten) business days from the sample provision date.
The expert assessment results for the PPE samples shall be an integral part of the expert report for assessment of a Bidder's technical proposal.
  Incoming inspection of PPE RS and delivered PPE shall be made successively for the following stages:
Stage 1 - identification of RS and PPE;
The PPE RS shall be identified in accordance with the requirements of the Uniform Industry Methodological Guidelines for performing incoming inspection of personal protective equipment used in the Rosatom State Corporation organizations No. 1/1354--P dated 23.06.2024
Stage 2 - verification of accompanying and operating documentation;
At this stage, the following verification work is carried out:
availability of the complete package of accompanying and operating documents, including certificates of compliance with the PPE, PPE test reports, PPE datasheets, operating manuals for the PPE and other documents specified in the contract for delivery of the PPE, including package of documents on the PPE RS;
Stage 3 - visual-instrumental control of PPE;
The visual and instrumental control of the PPE RS may be performed simultaneously, including after the control washing/decontamination of the RS (if the terms of the procurement documentation provide for the control washing/decontamination).
Stage 4 - PPE tests (if any);
Tests of RS at the TF (TL) are performed in accordance with the requirements of the
Uniform Industry Methodological Guidelines for incoming inspection of
personal protective equipment used in the Rosatom State Corporation organizations
No. 1/1354--P dated 23.06.2024 
In the event that the  conformity of the values of protective and other indicators of the provided RS with the
regulatory values specified in the technical assignment and
procurement documentation for delivery of PPE is not confirmed, the committee on incoming inspection of PPE, the Buyer shall take the decision on non-conformance of the RS with the requirements for the procured goods specified n the procurement documentation.
Stage 5 - issuance of the results of incoming inspection of RS and PPE.
The results of the PPE RS verification, including the results of the RS identification, verification of accompanying and operating documentation verification, visual and instrumental control, as well tests of RS at the TL (TC) shall be recorded in the PPE reference sample test report. If the results of the verification reveal non-conformance of the PPE RS with the requirements for the purchased goods specified in the procurement documents, the incoming inspection commission of the PPE shall draw up an act on the established discrepancy in quantity and quality when accepting the commodities and materials.
At the discretion of the committee (if necessary), samples may be submitted to accredited laboratories for additional testing when summarizing this procurement procedure.

PPE RS storage and return procedure:
The samples of each item of goods of the Bidders shall remain at the disposal of the Buyer at the end of the expert review procedure. If necessary, the PPE samples shall be returned to the bidders after summing up the procurement procedure following a written request from the Bidder addressed to the procurement procedure supervisor - Tamara Yylmaz T.Yilmaz@akkuyu.com. The request must contain the name of the Bidder, the list of samples to be returned and the full postal address for sending them. Returns shall be made by and at the expense of the Bidders.
The Commission for Incoming Inspection of PPE of the Corporation's organization after completion of the procurement procedure shall place the following in safe storage for subsequent return to the bidders:
PPE RS which were classified as not conforming with the requirements for the procured goods specified in the procurement documentation (not passing verification);
PPE RS, which successfully passed the verification, but were provided by the bidders, who following the verification were not identified as a supplier under the contract for delivery of the goods.
The PPE RS that were verified at the procurement procedure stage and provided by the bidder with whom the contract for procurement has b is concluded as a contract for the delivery of goods, remain in the organization of the Buyer as RS to perform incoming inspection of the PPE and are stored in places designated for storage of the PE, within the time limits set out during the procurement.
The deadline for return of the PPE RS to the bidder from the date on which the final report is posted on the official website (in the case of closed procurement - from the date of signing of the final report), on the basis of which the contract is concluded.

The Bidder, who had not submitted all the samples requested according to the list in Appendix 1 to the Assignments shall be rejected, as well as the Proposal by a Bidder that contains non-conformances of the samples provided with these Technical Requirements.
The dimensions of the goods are specified in accordance with Appendix 1 to the Technical Assignment 




SECTION 16. REQUIREMENTS TO QUANTITY, PLACE AND TERM (FREQUENCY) OF DELIVERIES
	In case of delivery of Goods to the Republic of Türkiye from abroad, the Goods shall be supplied under the terms of DDP Mersin, Türkiye, and after customs clearance, delivery to the place of destination shall be carried out by the Supplier, at the Supplier's own expense and by the Supplier's own efforts.
Place of delivery of the Goods: Republic of Türkiye, Büyükeceli quarter, Akkuyu street No. 3-A, Gülnar/Mersin.
The term of delivery of Goods shall be calculated from the date of the Contract conclusion.
The Goods shall be delivered in batches on the basis of Orders from the Buyer, sent in accordance with the form established by Appendix 7 to the concluded Contract. The Supplier is obliged to immediately confirm receipt of each Request and within 2 (two) working days from the date of receipt of the Buyer’s Request, the Supplier undertakes to deliver the Goods within 30 (thirty) calendar days from the date of receipt of the Buyer’s Request
Delivery of the Goods shall be carried out strictly on weekdays (from Monday to Friday) from 10.00 a.m. to 04.00 p.m. 



SECTION 17. REQUIREMENTS FOR THE FORM OF INFORMATION TO BE SUBMITTED
	The documents shall be submitted in Russian, Turkish and/or English.


SECTION 18. REQUIREMENTS FOR TECHNICAL TRAINING OF CUSTOMER'S PERSONNEL
	No requirements are established.


SECTION 19. LIST OF ABBREVIATIONS
	Item No.
	Abbreviation
	Key to abbreviations

	1. 
	TA
	Technical Assignment

	2. 
	PPE
	Personal Protective Equipment

	3. 
	(EN, ISO, TSE).
	Compliance with current European or Turkish standards

	4. 
	RS 
	Reference Specimen

	5. 
	TF 
	Testing Facility, accredited for carrying out
tests of PPE

	6. 
	TL
	Testing Laboratory, accredited for
conducting tests of PPE



SECTION 20. LIST OF APPENDICES
	Item No.
	Appendix  name
	Number 
of sheets

	1.
	Specification of Goods
	5

	2. 
	Requirements for the application of Company's logo
	1

	3
	Form of sample evaluation
	3

	4
	Letter form for provision of RS 
	1



2

                                                                                                                                     








                                     



                                    


                                   



















										      Annex No. 2 to the  
                                     Technical Assignment 
          
Requirements for applying Company's logos

No. 1 Logo to be located on color surfaces:
 
[image: ]





White logo (Pantone White), background - helmet color in accordance with the technical assignment 
The size of the logo is calculated in proportion to the height of the trade mark 
(without cipher margin) = 25 mm
Location: front side of the helmet in the form of sticker on transparent film

No. Logo  intended for placement on white surfaces:

[image: ]






Full-color logo, background - helmet color according to the Terms of Reference 
The size of the logo is calculated in proportion to the height of the trade mark 
(without cipher margin) = 30 mm
Location: front side of the helmet in the form of sticker on transparent film









Annex No. 3 
to the Technical Assignment
        Form of sample evaluation
     submitted by the Bidder for compliance with the Customer's requirements
                                                                                                            No.
Table 1
	No.
	Phases
	Complies /
does not comply 
	Comments
	Note

	1
	2
	3
	4
	5

	1
	Identification of delivered RS and PPE

	1.1
	Identification of delivered PPE/ PPE RS
	
	
	

	
	Indicators
	Name
	
	
	

	
	
	Article, model, brand
	
	
	

	
	
	Number 
	
	
	

	
	
	Size range
	
	
	

	1.2
	Identification of the PPE/PPE RS manufacturer
	
	
	

	
	Indicators
	Name
	
	
	

	
	
	Address (city)
	
	
	

	
	
	Place of production
	
	
	

	2
	Verification of accompanying and operating documentation

	
	Indicators
	PPE Сertificate of conformity 
	
	
	

	
	
	PPE Test protocols
	
	
	

	
	
	PPE operation manuals
	
	
	

	
	
	PPE manufacturer's data sheet
	
	
	

	
	
	Compliance with the protective properties of PPE 
	
	
	

	
	
	Warranty compliance 
	
	
	

	3
	Verification of the presence and integrity of proper packaging of PPE and PPE RS

	
	Indicators
	Availability of packing
	
	
	

	
	
	Integrity of packing
	
	
	

	
	
	Conformity of packing
	
	
	

	
	
	Conformity of content in packing 
	
	
	




	4
	Verification of the appearance (quality of PPE manufacture)

	
	Indicators
	Defects identified
	
	
	

	
	
	Conformance with models
	
	
	

	
	
	Conformance with sizes/heights
	
	
	

	
	
	Conformance with the color
	
	
	

	
	
	Conformance with the purpose
	
	
	

	
	
	Completeness
	
	
	

	5
	PPE visual and instrumental control

	
	Indicators
	Appearance
	
	
	

	
	
	Linear sizes
	
	
	

	
	
	Weight
	
	
	

	
	
	Thickness of protective material
	
	
	

	
	
	……
	
	
	

	6
	Checking of PPE marking

	6.1
	Marking on PPE
	
	
	

	6.2
	Marking on PPE packing
	
	
	

	6.3
	Conformity of information
	
	
	

	7
	PPE tests at the TF (TL)

	
	Indicators
	…
	
	
	

	
	
	…
	
	
	

	
	
	…
	
	
	


CONCLUSION

[bookmark: _Hlk161241573]Products (batch)    under No.                                   
(name or index)


meets the requirements 
(Document designation)

accepted and fit for purpose.

Products (lot)      under No.                                                              
(name or index)


do not meet the requirements 
(Document designation)

and shall be returned to the bidder, on the basis of a written request addressed to the initiator of the procurement procedure, Tamara Yilmaz , for the purpose of correcting the identified discrepancies on the basis of (Act of Established Discrepancies in Quantity and Quality upon Acceptance of goods and materials No. _____ dated _____ or on the basis of Supplier’s Letter of Agreement No. ____ dated ________ specifying the replacement period of the non-conforming PPE) 
Division Manager, 
performing incoming inspection
  Initials, last name
	20	.                                                                          

                                                                Annex No. 4
to the Technical Assignment
  
AKKUYU NÜKLEER ANONİM SIRKETI


Dear Mr., 

In accordance with the requirements of the Specification and as part of the ongoing procurement procedure, we hereby notify the sending of test samples of the goods for verification and conformity assessment.
List of provided reference samples:
Delivery date and delivery time__________________________  
1.	Position No. ________________
Name: __________________________
Quantity: __________________________pcs.
2.	Position No. ________________
Name: __________________________
Quantity: _____________________________pcs.
Supporting documentation for refefence specimen:
•	Certificates of conformity indicate which items, if any);
•	Test reports (if any);
•	Quality Certificates (indicate quantity and position, if available).
All test samples provided correspond to the stated specifications and requirements of the Technical Specification.

Yours sincerely, 
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